**Architype Code:** A-B-B-A-A-A-C **Number of Dwellings like this in England:** 68717

**Building Type:**

**Wall Construction:** Soild Masonry **Floor Construction:** Suspended Timber Floor

**Roof Type:** Pitched no attic **Roof Suitable for Solar Panels:** Yes

**Double Glazing:** Entire house

**Energy System:** Gas central heating & Water, with hot water tank

**Dwellings like this are typically:**

Built between: 1909 - 1933

Usable Floor area (m2): 68 - 123

SAP Energy Rating: 41 - 57

Number of Windows: 10 - 20

Number of external Doors: 2 - 2

Percentage with access to mains gas: 100 %

Maximum roof area that could be used for solar panels (m2):

Percentage with well insulated hot water tank: 0

Typical Heating Controls: 5 - 5

Typical Radiator Controls: 1 - 2