**Architype Code:** A-B-B-A-A-A-C **Number of Dwellings like this in England:** 68717

**Building Type:** Semi Detached/End Terrace **Double Glazing:** Entire house

**Wall Construction:** Soild Masonry **Floor Construction:** Suspended Timber Floor

**Roof Type:** Pitched no attic **Roof Suitable for Solar Panels:** Yes

**Energy System:** Gas central heating & Water, with hot water tank

**Dwellings like this are typically**

|  |  |  |  |
| --- | --- | --- | --- |
| Desciption | Value | Desciptions | Values |
| Built between | 1909 - 1933 | Usable Floor area (m2) | 68 - 123 |
| SAP Energy Rating | 41 - 57 | Max Solar Area | 11 - 21 |
| Number of Windows | 10 - 20 | Number of external Doors | 2 - 2 |
| Heating Controls | 5 - 5 | Radiator Controls | 1 - 2 |
| % with insualted tank | 0 | % with access to mains gas | 100 |

**Most Common Locations**

|  |  |
| --- | --- |
| locations | percent |
| suburban residential | 57 |
| other urban centre | 20 |